                                                                     1997
                      WL2420, WL2430 WIRELESS LAN CARD

1. Wl2420P.COM, Packet Driver for ISA Card

        Syntax : WL2420P.COM [-u] <packet_int_no>

        For example, to load packet driver on vector 0x60 :

                C:> WL2420P 0x60

        For example, to unload packet driver :

                C:> WL2420P -u 0x60


2. Wl2430P.COM, Packet Driver for PCMCIA Card

        Syntax : WL2430P.COM [-u] <packet_int_no>

        For example, to load packet driver on vector 0x60 :

                C:> WL2430P 0x60

        For example, to unload packet driver :

                C:> WL2430P -u 0x60



Notes:

<packet_int_no> is the software interrupt vector number used by the
                packet driver program, which can be from 96 (0x60)
                to 128 (0x80).

[-u]            Uninstall packet driver.




